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The comparison between the index of diesel, mixed oil after distillation and international standard 0# diesel

	Item
	Diesel (after distillation)
	Mixed oil
	international standard 0# diesel

	oxidation stability
	2.0
	1.5
	2.5

	sulfur content %
	0.005
	0.005
	0.05

	10%residue %
	0.25
	0.2
	0.3

	ash content %
	0.008
	0.007
	0.01

	copper corrosion /rank
	1.1
	1.1
	1

	Water content%
	mark
	mark
	mark

	mechanical impurity
	no
	no
	no

	density
	0.85
	0.80
	0.82-0.86

	Solidifying point /℃
	-10
	-20
	0

	flashing point (close)/℃
	45
	40
	55

	Kinetic viscosity
	2.5
	2.0
	3.0-8.0

	Combustion value KJ/ kg
	9500
	9200
	8500

	chrominance
	1.2
	1.5
	≤3.5

	cetane ratio
	43
	40
	46
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