EXPERIMENT I: Relationship of change in frequency of oscillations with change in flow rate when height of bladder from ground is constant
	Flow rate in ml/sec
	Freq of collapse per min

	Pressure at inlet in mm Hg

	Max pressure at outlet in mm Hg
	Min pressure at outlet in mm Hg
	Range of pressure

fluctuations in mm Hg
	Average velocity of flow in m/sec

	146

	108
	-7

	-116

	-154

	37

	1.2


	200

	100

	-9

	-122

	-158

	37

	1.8


	250

	74
	-10
	-1456

	-196

	50

	2.2


	278

	80

	-7

	-94

	-150

	56

	2.5


	303

	62
	-9

	-112

	-150

	38

	2.5


	332
	52
	-7

	-100.

	-127

	26

	2.6


	435
	30
	-9

	-146

	-176

	30

	2.9



	


