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Magnetic Three Layer Electromechanical Movement technology

i Motors
conventional Figure 1 and 2 show what I call two layer electromechanical movement. It is a rotor

N have one
motor has two ermanent operating with a stator. Figure one shows the electric motors that are built with
conventional l‘M torque with all electromagnets. Figure 2 shows magnetic motors currently used in
electomagnets agnet cars having one permanent magnet per one electromagnet. You have magnetic

and one motors in electric cars over electric motors because you get better range from those
electromagnet mote

5 Figure 3 shows the two of the four segments of travel in a Three Layer
Figure 1 Figure 2 Electromechanical Movement technology. Both part 1 and part 2 move the same
distance in a motor. Part 1 does not require any electricity in order for the magnets
to align each other through attraction. In part 2, the electromagnet is activated as
Part 1 Part 2 is shown in figure 4 in order to produce a functional magnet. When the power is
supplied to the electromagnet the functional magnet is activated and when the

N N power is turned of it gone as far as the magnetic fields go because the coil has an air
Rotor 1 s Rotor 1 core.
N

S Part 1 and Part 2 repeat themself with a different
EM oy electromagnet circuit in parts 3 and 4 in order to complete the

PM1
Stator N N

four segments of travel of the rotors moving through the stator
assembly. When you add up the torques from each parts of
s s Part 1 and Part 2, they add up to torque from 5 PMs to 1 EM.

N
Even if you caluculate less than I do, the torque ratio is better
N |. Rofor 2 Functional than the current magnetic moros used in cars today. THis
N

Maguet technology needs to be explored. Please help me out in
Dringing this technology into reali
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